**Anti-foam Job Aid**

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

To get the anti-foam script you can either retrieve the Auto feed script with anti-foam or just ant-foam.





When the anti-foam script starts and is working correctly it will say: 24-hour anti-foam shot counter reset.







When the foam hits the sensor probe it will read out: “Foam rising, starting anti-foam.” The anti-foam will have a 1-minute delay before dispensing the anti-foam and once it is dispensing the anti-foam it will read out: “Dispensing anti-foam.”







When a shot is dispensed it will note down how much it is dispensed in mL it will also let you know what number shot this is. And then finally start a 1-hour post-shot delay to let the foam level reduce when the anti-foam is dispensed.





This message means that the 1-hour delay is complete, after this it will reset the state. This means that it will go back to the original state where the foam level is low and it will say no anti-foam is needed.



When “the number of shots reached” reaches a number of 5 shots it will display this message, meaning that it reached the maximum number of shots and will not dispense any more shots of anti-foam.



Then after 24 hours of the start of the inoculation timer it will read this message. This means that the number of shots will equal zero and it will be able to dispense more anti-foam shots when needed.